Configuration Name: HOSTMOT2

General configuration information:

  BoardName : MESA7I92
  FPGA Size: 20 KGates
  FPGA Pins: 256
  Number of IO Ports: 2
  Width of one I/O port: 17
  Clock Low frequency: 100.0000 MHz
  Clock High frequency: 175.0000 MHz
  IDROM Type: 3
  Instance Stride 0: 4
  Instance Stride 1: 64
  Register Stride 0: 256
  Register Stride 1: 256

Modules in configuration:

  Module: DPLL
  There are 1 of DPLL in configuration
  Version: 0
  Registers: 7
  BaseAddress: 7000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: WatchDog
  There are 1 of WatchDog in configuration
  Version: 0
  Registers: 3
  BaseAddress: 0C00
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: IOPort
  There are 2 of IOPort in configuration
  Version: 0
  Registers: 5
  BaseAddress: 1000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: QCount
  There are 2 of QCount in configuration
  Version: 2
  Registers: 5
  BaseAddress: 3000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: StepGen
  There are 10 of StepGen in configuration
  Version: 2
  Registers: 10
  BaseAddress: 2000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: PWM
  There are 2 of PWM in configuration
  Version: 0
  Registers: 5
  BaseAddress: 4100
  ClockFrequency: 175.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: LED
  There are 1 of LED in configuration
  Version: 0
  Registers: 1
  BaseAddress: 0200
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

Configuration pin-out:

IO Connections for P2
DB25 pin#             I/O   Pri. func    Sec. func        Chan     Sec. Pin func   Sec. Pin Dir

 1                      0   IOPort       None           
14                      1   IOPort       None           
 2                      2   IOPort       StepGen          0        Dir/Table2      (Out)
15                      3   IOPort       None           
 3                      4   IOPort       StepGen          0        Step/Table1     (Out)
16                      5   IOPort       StepGen          4        Step/Table1     (Out)
 4                      6   IOPort       StepGen          1        Dir/Table2      (Out)
17                      7   IOPort       PWM              0        PWM             (Out)
 5                      8   IOPort       StepGen          1        Step/Table1     (Out)
 6                      9   IOPort       StepGen          2        Dir/Table2      (Out)
 7                     10   IOPort       StepGen          2        Step/Table1     (Out)
 8                     11   IOPort       StepGen          3        Dir/Table2      (Out)
 9                     12   IOPort       StepGen          3        Step/Table1     (Out)
10                     13   IOPort       None           
11                     14   IOPort       QCount           0        Quad-A          (In)
12                     15   IOPort       QCount           0        Quad-B          (In)
13                     16   IOPort       QCount           0        Quad-IDX        (In)

IO Connections for P1
DB25 pin#             I/O   Pri. func    Sec. func        Chan     Sec. Pin func   Sec. Pin Dir

 1                     17   IOPort       PWM              1        PWM             (Out)
14                     18   IOPort       None           
 2                     19   IOPort       StepGen          5        Dir/Table2      (Out)
15                     20   IOPort       None           
 3                     21   IOPort       StepGen          5        Step/Table1     (Out)
16                     22   IOPort       StepGen          9        Step/Table1     (Out)
 4                     23   IOPort       StepGen          6        Dir/Table2      (Out)
17                     24   IOPort       PWM              1        PWM             (Out)
 5                     25   IOPort       StepGen          6        Step/Table1     (Out)
 6                     26   IOPort       StepGen          7        Dir/Table2      (Out)
 7                     27   IOPort       StepGen          7        Step/Table1     (Out)
 8                     28   IOPort       StepGen          8        Dir/Table2      (Out)
 9                     29   IOPort       StepGen          8        Step/Table1     (Out)
10                     30   IOPort       None           
11                     31   IOPort       QCount           1        Quad-A          (In)
12                     32   IOPort       QCount           1        Quad-B          (In)
13                     33   IOPort       QCount           1        Quad-IDX        (In)

