Configuration Name: HOSTMOT2

General configuration information:

  BoardName : MESA7I92
  FPGA Size: 20 KGates
  FPGA Pins: 256
  Number of IO Ports: 2
  Width of one I/O port: 17
  Clock Low frequency: 100.0000 MHz
  Clock High frequency: 175.0000 MHz
  IDROM Type: 3
  Instance Stride 0: 4
  Instance Stride 1: 64
  Register Stride 0: 256
  Register Stride 1: 256

Modules in configuration:

  Module: DPLL
  There are 1 of DPLL in configuration
  Version: 0
  Registers: 7
  BaseAddress: 7000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: WatchDog
  There are 1 of WatchDog in configuration
  Version: 0
  Registers: 3
  BaseAddress: 0C00
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: IOPort
  There are 2 of IOPort in configuration
  Version: 0
  Registers: 5
  BaseAddress: 1000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: QCount
  There are 6 of QCount in configuration
  Version: 2
  Registers: 5
  BaseAddress: 3000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: StepGen
  There are 5 of StepGen in configuration
  Version: 2
  Registers: 10
  BaseAddress: 2000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: PWM
  There are 1 of PWM in configuration
  Version: 0
  Registers: 5
  BaseAddress: 4100
  ClockFrequency: 175.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: LED
  There are 1 of LED in configuration
  Version: 0
  Registers: 1
  BaseAddress: 0200
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

Configuration pin-out:

IO Connections for P2
DB25 pin#             I/O   Pri. func    Sec. func        Chan     Sec. Pin func   Sec. Pin Dir

 1                      0   IOPort       PWM              0        PWM             (Out)
14                      1   IOPort       None           
 2                      2   IOPort       StepGen          0        Step/Table1     (Out)
15                      3   IOPort       None           
 3                      4   IOPort       StepGen          0        Dir/Table2      (Out)
16                      5   IOPort       StepGen          4        Step/Table1     (Out)
 4                      6   IOPort       StepGen          1        Step/Table1     (Out)
17                      7   IOPort       StepGen          4        Dir/Table2      (Out)
 5                      8   IOPort       StepGen          1        Dir/Table2      (Out)
 6                      9   IOPort       StepGen          2        Step/Table1     (Out)
 7                     10   IOPort       StepGen          2        Dir/Table2      (Out)
 8                     11   IOPort       StepGen          3        Step/Table1     (Out)
 9                     12   IOPort       StepGen          3        Dir/Table2      (Out)
10                     13   IOPort       None           
11                     14   IOPort       QCount           0        Quad-A          (In)
12                     15   IOPort       QCount           0        Quad-B          (In)
13                     16   IOPort       QCount           0        Quad-IDX        (In)

IO Connections for P1 -> HDR26
Pin#                  I/O   Pri. func    Sec. func        Chan     Sec. Pin func   Sec. Pin Dir

1                      17   IOPort       QCount           1        Quad-A          (In)
2                      18   IOPort       QCount           1        Quad-B          (In)
3                      19   IOPort       QCount           1        Quad-IDX        (In)
4                      20   IOPort       QCount           2        Quad-A          (In)
5                      21   IOPort       QCount           2        Quad-B          (In)
6                      22   IOPort       QCount           2        Quad-IDX        (In)
7                      23   IOPort       QCount           3        Quad-A          (In)
8                      24   IOPort       QCount           3        Quad-B          (In)
9                      25   IOPort       QCount           3        Quad-IDX        (In)
11                     26   IOPort       QCount           4        Quad-A          (In)
13                     27   IOPort       QCount           4        Quad-B          (In)
15                     28   IOPort       QCount           4        Quad-IDX        (In)
17                     29   IOPort       QCount           5        Quad-A          (In)
19                     30   IOPort       QCount           5        Quad-B          (In)
21                     31   IOPort       QCount           5        Quad-IDX        (In)
23                     32   IOPort       None           
25                     33   IOPort       None           

