o<touch_x> sub

#<set_mt_x> = #1    (current x axis position)
#<gage_thickness> = #2    (=0.0000)(gage thickness, gage block or paper thickness etc.)

G8

#<total_x_position> = [#<set_mt_x> + #<gage_thickness>]

#<current_tool_x_position> = #5420

#<touch_x> = [#<current_tool_x_position> - #<total_x_position>]

G10 L1 P #5400 X [#<touch_x>]  (5400 = tool number)

T #5400 G43 (enable tool length offset)

G7

o<touch_x> endsub

M2 (end program)
